
#comment ; #
#option_force_device=COM1        #please correct use of upper and lower case
option_auto_start=1              #Auto Start on every exynos port(device) one by one.
option_pause_before_terminate=0  #show 'press enter to exit' before program finished.
option_program_loop=1            #show 'press enter to refresh' and skip scanning instead program finishes.
option_stop_program_on_fail_response=1 #stop program if got nak or unexpected

send bl1 bl1_usb.signed
send EPBL pbl_usb.signed
send BL2 bl2.header
send BL2B bl2.body
send ABL abl.header
send ABLB abl.body
send BL31 bl31.header
send BL3B bl31.body
send GSA1 gsa_usb.signed
send TZSW trusty.header
send TZSB trusty.body
send LDFW ldfw.header
send LDFB ldfw.body
send DPM zero.bin
